

Product name: Buildon Bondit 151

Application :

 

Description :

BUILDON BONDIT 151 is high performance bonding agent for
 Gypsum on concrete blocks/RCC surfaces. Further it has waterproofing properties and hence it prevents leakages from
the cracks in the plaster.

Fields of application :

* Waterproof Coating
* CrackSealing
* Bonding of Gypsum
* Concrete Repairs
* Tile Fixing on walls
* Fixing Tile on Tile

Technical Specification:

|  |  |
| --- | --- |
| Chemical Composition | Modified Hybrid System. |
| Physical Appearance | Milky White Emulsion |
| Solid Contents | More than 40% |
| Viscosity | 1500 cps Max |
| PH Value | 7 - 9 |
| Butt joint strength | 2000gsm/scm |
| Film Characteristics | Clear, forms flexible system with cement |
| Handling & Storage | Protect from frost. Containers once opened should be shut tightly to prevent contamination. Stocks should be used on a first in, first out basis. |
| Packing | 20 kgs HDPE Jerry cans |

* Clean the Concrete Surface with water to remove dust and de-moulding compound.
* Apply Bondit-151 with brush or spray machine.
* Within 30 minutes when Bondit-151 is tacky apply gypsum plaster.

ASTM & Code Standards:

:

* N/A

Shelf Life :

:

* Six months from Date of Manufacturing

Technical Assistance :

Buildon

3b ,Mapkhan Compound, Mapkhan Nagar, Marol Maroshi Road, Andheri – East, Mumbai – 400059.

Tel : +91 65345120/+91 43471098
Email : buildonindia@gmail.com

Website : www.buildon.co.in